emco Bau Logo

**emco Bau**

emco DIPLOMAT Premium Large With Outdoor insert and brush strip 522 PL Outdoor B

|  |  |
| --- | --- |
| **Model** | 522 PL Outdoor B |
| **Load** | Normal to heavy |
| **Support chassis** | Made using aluminium with sound absorbing insulation on the underside |
| **Support chassis colour** | Anodised colours for an additional charge: EV3 gold, C33 mid-bronze, C35 black or C31 stainless steel |
| **Approx. height (mm)** | 22 |
| **Tread surface** | The weather-resistant Outdoor insert for noticeably thorough removal of coarse dirt. The additional profile increases the cleaning power. |
| **Standard profile clearance approx. (mm)** | 5 mm, rubber spacers |
| **Revolving door drives** | Our mats with a profile spacing of 3mm in accordance with DIN EN 16005 are available for revolving door drives. |
| **Colours** | Anthracite |
|  | Brown |
|  | Red |
|  | grey |
|  | Black |
| **Flammability** | Insert with fire classification Cfl-s1 according to EN 13501. |
| **Connection** | Thanks to plastic-coated steel cable |
| **Warranty** | 5 years guarantee |
|  | Warranty conditions are available at: |
| **Pile material** | 100% PA 6 (polyamide) |
| **Use classification EN1307** | Property suitable inlay 33 |
| **Dimensions** | Mat width:.........................mm (bar length) |
|  | Mat depth:.........................mm (walking direction) |
| **BIM Data** | BIM Data is available to download from https://www.emco-bau.com/pim/bim-daten-GER.zip. |
| **Contact** | emco Bautechnik GmbH · Breslauer Straße 34 - 38 · D-49808 Lingen (Ems) Germany · Phone: +49 (0) 591/9140-500 · Fax: +49 (0) 591/9140-852 Email: bau@emco.de · www.emco-bau.com |