

**emco Bau**

emco MARSCHALL Premium With Maximus Image insert and brush strip 522 PS Maximus Image B

|  |  |
| --- | --- |
| **Model** | 522 PS Maximus Image B |
| **Load** | Extremely heavy |
| **Support chassis** | Reinforced support chassis made using rigid aluminium with sound absorbing insulation on the underside |
| **Support chassis colour** | Anodised colours for an additional charge: EV3 gold, C33 mid-bronze, C35 black or C31 stainless steel |
| **Approx. height (mm)** | 22 |
| **Tread surface** | Embedded, robust MAXIMUS inserts in Bfl-S1 quality (clean-off floor covering made from special polyamide yarn, 100%) |
| **Standard profile clearance approx. (mm)** | 5 mm, rubber spacers |
| **Revolving door drives** | Our mats with a profile spacing of 3mm in accordance with DIN EN 16005 are available for revolving door drives. |
| **Colours** | I350 Blue grey |
|  | I80 Bordeaux |
|  | I260 Brown |
|  | I380 Dark grey |
|  | I210 Dark green |
|  | I120 Lilac |
|  | I30 Yellow/orange |
|  | I20 Yellow |
|  | I420 Gold |
|  | I270 Graphite |
|  | I340 Grey beige |
|  | I370 Grey |
|  | I250 Green |
|  | I170 Light blue |
|  | I360 Light grey |
|  | I440 Light green |
|  | I90 Light red |
|  | I100 Cherry |
|  | I430 Salmon pink |
|  | I230 Leaf green |
|  | I290 Light blue |
|  | I110 Purple |
|  | I140 Magenta |
|  | I200 Marine blue |
|  | I330 Chestnut |
|  | I220 Mint |
|  | I40 Orange |
|  | I70 Oxide red |
|  | I180 Petrol blue |
|  | I150 Peach |
|  | I310 Fawn brown |
|  | I60 Red |
|  | I160 Royal blue |
|  | I320 Sand |
|  | I240 Reed green |
|  | I390 Black |
|  | I300 Silver |
|  | I190 Emerald green |
|  | I280 Steel blue |
|  | I410 Steel grey |
|  | I450 Sunset |
|  | I50 Terracotta |
|  | I130 Grape |
|  | I400 White\* |
|  | I10 Lemon |
|  | grey |
|  | Black |
| **Special colours** | Other colours from our clean-off collection also available. |
| **Flammability** | Insert with fire classification Bfl-s1 according to EN 13501. |
| **Connection** | Plastic-coated steel cable |
| **Warranty** | 5 years guarantee |
|  | Warranty conditions are available at: |
| **Pile material** | 100% PA 6.6 (polyamide) |
| **Use classification EN1307** | Property suitable inlay 33 |
| **Dimensions** | Mat width:.........................mm (bar length) |
|  | Mat depth:.........................mm (walking direction) |
| **BIM Data** | BIM Data is available to download from https://www.emco-bau.com/pim/bim-daten-GER.zip. |
| **Contact** | emco Bautechnik GmbH · Breslauer Straße 34 - 38 · D-49808 Lingen (Ems) Germany · Phone: +49 (0) 591/9140-500 · Fax: +49 (0) 591/9140-852 Email: bau@emco.de · www.emco-bau.com |